Set up of LAN Segments

Introduction

**Objective**

At the end of this guide, you will learn how to configure network interfaces.

**Login**

The login credential for all server and client machines:

Username: root / user

Password: Skill39@Lyon

**Network Topology**

Create 3 LAN Segments:

INT

DMZ

WAN

vim /etc/network/interfaces